**RAIN GARDEN NOTES**

***Unless Otherwise Noted***

1. Rain garden grading and bottom area must be as shown on the approved plan. Subgrade must be scarified 4 inches minimum. Soil must be compost amended for 12 inches minimum or 12 inches minimum of bioretention soil must be placed. Imported bioretention soil, if used, must be per Specification 9-14.1(4).
2. If shown on the approved plan, berm material must be the same as rain garden soil mounded a minimum of 2 inches above finished grade and compacted to 90% dry density.
3. Arborist wood mulch must be per Specification 9-14.4(4). Finished grade must be one inch below walks and curbs.
4. Rain garden landscaping must be as shown on the approved plan. Changes to the approved landscaping plan require submittal of a revised landscaping plan.
5. After planting, rain gardens must be inspected and approved by the City of Seattle, or an approved representative.
6. Protect all rain gardens from accumulating sediments and compaction. Any impacted rain garden must be restored to fully functioning condition by removal of sediment laden soils, over excavation as approved the City of Seattle, or an approved representative and replacement with new bioretention soil per Specification 9-14.1(4).
7. Water to ensure vegetation survival.